Router>en

Router#conf t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#int fa0/0

Router(config-if)#ip adress 192.168.0.2.255.255.255.0

Router(config-if)#ip address 192.168.0.1.255.255.255.0

^

% Invalid input detected at '^' marker.

Router(config-if)#ip address 192.168.0.1 255.255.255.0

Router(config-if)#no shutdown

Router(config-if)#

%LINK-5-CHANGED: Interface FastEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/0, changed state to up

Router(config-if)#do write memory

Building configuration...

[OK]

Router(config-if)#ip dhcp pool net1

Router(dhcp-config)#network 192.168.0.1 255.255.255.0

Router(dhcp-config)#exit

Router(config)#int fa0/1

Router(config-if)#ip address 192.168.1.1 255.255.255.0

Router(config-if)#no shutdown

Router(config-if)#

%LINK-5-CHANGED: Interface FastEthernet0/1, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up

Router(config-if)#do write memory

Building configuration...

[OK]

Router(config-if)#ip dhcp pool net2

Router(dhcp-config)#network 192.168.1.1 255.255.255.0

Router(dhcp-config)#exit

Router(config)#

Router#

%SYS-5-CONFIG\_I: Configured from console by console

Router#